{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":71,"n_cols":3,"rows_kept":71,"cut":false,"hidden":false,"merged":[]}
["Description","Title","Total\nQTY"]
["DIN 25201 - M10 - A4-\n80","Nord-Lock Washer",120]
["DIN 25201 - M10 - A4-80","Nord-Lock Washer",60]
["DIN 25201 - M10 - St - \nHDG","Nord-Lock Washer",90]
["DIN 25201 - M12 - A4-80","Nord-Lock Washer",30]
["DIN 25201 - M12 - St - \nHDG","Nord-Lock Washer",30]
["DIN 25201 - M12sp - St - \nHDG","Nord-Lock Washer",30]
["DIN 25201 - M14 - St - \nHDG","Nord-Lock Washer",15]
["DIN 25201 - M14sp - St - \nHDG","Nord-Lock Washer",15]
["DIN 25201 - M24 - St - HDG","Nord-Lock Washer",0]
["DIN 25201 - M6 - A4-80","Nord-Lock Washer",90]
["DIN 25201 - M8 - A4-80","Nord-Lock Washer",180]
["DIN 25201 - M8 - St - HDG","Nord-Lock Washer",90]
["DIN 580 - M20 x 30 - \nC15E - HDG","Eye Bolt",15]
["DIN 6885 Form B 10x8x20","Parallel keys",3]
["DIN 6885 Form B 10x8x50","Parallel keys",3]
["DIN 6885 Form B 12x8x50","Parallel keys",3]
["DIN 7984 - M8 x 25 x \n21.25 - 8.8 - HDG","Hex Socket Head Cap Screw Low",15]
["DIN 913 - M6 x 16 - A4","Hexagon Socket Set Screw Flat Point",6]
["DIN 913 - M6 x 8 - A4","Hexagon Socket Set Screw Flat Point",9]
["ISO 10642 - M10 x 35 x 35 \n- A4-80","Hex Socket Countersunk Head Screw",30]
["ISO 4017 - M10 x 25 - 8.8 - \nHDG","Hex Head Screw",30]
["ISO 4017 - M10 x 40 - 8.8 - \nHDG","Hex Head Screw",105]
["ISO 4017 - M10 x 45 - 8.8 - \nHDG","Hex Head Screw",15]
["ISO 4017 - M10 x 65 - A4-80","Hex Head Screw",30]
["ISO 4017 - M12 x 30 - 8.8 - \nHDG","Hex Head Screw",120]
["ISO 4017 - M12 x 50 - 8.8 - \nHDG","Hex Head Screw",30]
["ISO 4017 - M12 x 90 - 8.8 - \nHDG","Hex Head Screw",15]
["ISO 4017 - M14 x 35 - 8.8 - \nHDG","Hex Head Screw",15]
["ISO 4017 - M16 x 50 - 8.8 - \nHDG","Hex Head Screw",0]
["ISO 4017 - M24 x 65 - 8.8 - HDG","Hex Head Screw",0]
["ISO 4017 - M24 x 90 - 8.8 - HDG","Hex Head Screw",90]
["ISO 4017 - M30 x 90 - 8.8 - HDG","Hex Head Screw",30]
["ISO 4017 - M6 x 16 - A4-\n80","Hex Head Screw",45]
["ISO 4017 - M8 x 25 - A4-\n80","Hex Head Screw",60]
["ISO 4017 - M8 x 30 - 8.8 - \nHDG","Hex Head Screw",30]
["ISO 4017 - M8 x 35 - 8.8 - \nHDG","Hex Head Screw",150]
["ISO 4017 - M8 x 60 - 8.8 - \nHDG","Hex Head Screw",15]
["ISO 4032 - M10 - 8 - HDG","Hex Nut",60]
["ISO 4032 - M12 - 8 - HDG","Hex Nut",30]
["ISO 4032 - M14 - 8 - HDG","Hex Nut",15]
["ISO 4032 - M24 - 8 - HDG","Hex Nut",165]
["ISO 4032 - M30 - 8 - HDG","Hex Nut",30]
["ISO 4032 - M6 - A4-80","Hex Nut",30]
["ISO 4032 - M8 - 8 - HDG","Hex Nut",45]
["ISO 4762 - M10 x 35 x 35- \nA4-80","Hex Socket Head",30]
["ISO 4762 - M10 x 65 x 32- A4-80","Hex Socket Head",0]
["ISO 4762 - M12 x 55 x 36- \nA4-80","Hex Socket Head",30]
["ISO 4762 - M12 x 65 x 36 - \n8.8 - HDG","Hex Socket Head",30]
["ISO 4762 - M14 x 80 x 40 - \n8.8 - HDG","Hex Socket Head",30]
["ISO 4762 - M16 x 40 x 40- \nA4-80","Hex Socket Head",15]
["ISO 4762 - M4 x 40 x 20- \nA4-80","Hex Socket Head",30]
["ISO 4762 - M5 x 12 x 12- \nA4-80","Hex Socket Head",30]
["ISO 4762 - M6 x 20 x 20- \nA4-80","Hex Socket Head",30]
["ISO 4762 - M8 x 70 x 28 - \n8.8 - HDG","Hex Socket Head",30]
["ISO 7040 - M10 - A4-80","Prevailing Torque Nut",30]
["ISO 7040 - M12 - 8 - HDG","Prevailing Torque Nut",15]
["ISO 7040 - M4 - A4-80","Prevailing Torque Nut",15]
["ISO 7089 - M10 - HV200 - \nHDG","Washer",30]
["ISO 7089 - M12 - HV200 - \nHDG","Washer",210]
["ISO 7089 - M14 - HV200 - \nHDG","Washer",15]
["ISO 7089 - M16 - HV200 - \nHDG","Washer",15]
["ISO 7089 - M24 - HV200 - HDG","Washer",180]
["ISO 7089 - M30 - HV200 - HDG","Washer",60]
["ISO 7089 - M4 - A4-HV200","Washer",30]
["ISO 7089 - M5 - HV200 - \nHDG","Washer",15]
["ISO 7089 - M6 - A4-HV200","Washer",30]
["ISO 7089 - M8 - HV200 - \nHDG","Washer",15]
["ISO 7090 - M12 - HV300 - \nHDG","Washer",30]
["ISO 7090 - M8 - HV300 - \nHDG","Washer",30]
["ISO 7093 - M12 - HV200 - \nHDG","Large Washer",15]